**SPECIFICATIONS FOR 8.3MM LAMINATE**

|  |  |
| --- | --- |
| **QUANTITY PER BOX** | **20.56 SQFT/ 1.9101SQM** |
| **PIECES PER BOX** | **8** |
| **DIMENSIONS** | **1212 x 197 x 8MM**  **(47.7 x 7.76 x 1.33)** |
| **CERTIFICATION** | **ISO 9001**  **ISO 14001** |
| **RATING** | **AC3/CLASS 31** |
| **WEIGHT** | **15.2 kg/box** |
| **CARB COMPLIANCE** | **PHASE 1: 0.21 PPM**  **(CALIFORNIA STANDARD)** |