**Specifications for Sound Solution XPE**

* Water Proof as moisture barrier
* Will absorb and reduce the transmission of noise associated with normal foot traffic
* High density & tear strength

**Materials**

* Black Foam with Aluminum Foil

**Package**

* 200 sf/roll
* 3mm thickness

**Moisture Resistance**

* 98%

STC = 55

HC= 58

IIC = 56